

**Flash BIOS in EFI shell:**


1. Ensure the USB drive is in FAT32 format. if not, format it to FAT32.
2. Extract the UEFI shell to the root directory of the USB drive, and copy the BIOS flash package to the USB drive.
3. Power on and press F7 pop menu to select boot from the USB UEFI shell.



1. Select the FS where the USB drive is located. For example, the USB drive is FS0 as shown in the figure below.




1. Execute the batch file efiflash.nsh in the BIOS package



6.On the first boot after flash BIOS, Please press DEL to enter BIOS Setup and load defaults.

**Flash BIOS in Windows:**

1. Double-click WinFlash.bat in the BIOS package. Do not perform any other operations during the update. The system will restart automatically after the update is completed.



2.On the first boot after flash BIOS, Please press DEL to enter BIOS Setup and load defaults .