!!!Warning!!! Do not turn off the power when flashing!!!!!!!!!!!!
This is a non-public beta BIOS. For testing purposes only, please do not disclose it to others.


Universal BIOS FLASH.

A. Windows 

1. Disable "secure boot" in BIOS
2. Run as administrator run "AfuWinFlash.bat"


B. In BIOS UEFI SHELL

1. Unzip file to root of FAT32 format disk.
2. Disable "secure boot" in BIOS
3. Boot into U disk, with uefi shell(F7 to choose boot disk)
3. Use "FS1:" "FS2:" to find your BIOS udisk. (you can use command "ls" to check files exists)
4. Run AfuEfiFlash.nsh.
